## Atheros Client Utility Help

Introduction

- System Requirements

Profile Management

- Create or Modify a Profile

- Remove a Profile

- Profile Auto Selection

- Switch Profiles

- Configure TCP/IP

- Configuring Win XP

Security

- EAP-TLS

- EAP-TTLS

- PEAP (EAP-GTC)

- PEAP (EAP-MSCHAP V2)

- LEAP

- WPA Passphrase

Check Status or Diagnostics

- Check Current Status

- Check Driver Information

- Check Statistics

Connect to Another Network

Settings

- Signal Strength Display

- Data Display

- Display Refresh Interval

Tools

- Tray Icon

- Troubleshooting Utility

- Enable/ Disable the Radio

### ACU Tools

Use the Action menu to access the Atheros Client Utility tools:

Enable/Disable Radio | Enable or disable the RF Signal on all Atheros station reference designs.
Enable/Disable Tray Icon | Enable or disable the tray icon.
Troubleshooting | Run the optional Troubleshooting Utility.
Manual LEAP Login | Log in to LEAP manually, if LEAP is set to manually prompt for user name and password on each login.
Reauthenticate | Reauthenticate to a LEAP-configured access point.
Exit | Exit the Atheros Client Utility application.