## Atheros Client Utility Help

Introduction

- System Requirements

Profile Management

- Create or Modify a Profile

- Remove a Profile

- Profile Auto Selection

- Switch Profiles

- Configure TCP/IP

- Configuring Win XP

Security

- EAP-TLS

- EAP-TTLS

- PEAP (EAP-GTC)

- PEAP (EAP-MSCHAP V2)

- LEAP

- WPA Passphrase

Check Status or Diagnostics

- Check Current Status

- Check Driver Information

- Check Statistics

Connect to Another Network

Settings

- Signal Strength Display

- Data Display

- Display Refresh Interval

Tools

- Tray Icon

- Troubleshooting Utility

- Enable/ Disable the Radio

### Profile Management

Configure the wireless network adapter (wireless card) from the Profile Management tab of the Atheros Client Utility.

- Add a profile
- Edit a profile
- Import a Profile
- Export a Profile

- Order profiles
- Switch to a different profile
- Remove a profile
- Connect to a Different Network

The wireless network adapter works in either infrastructure mode (which uses an access point) or ad hoc mode (a group of stations participating in the wireless LAN).