## Atheros Client Utility Help

Introduction

- System Requirements

Profile Management

- Create or Modify a Profile

- Remove a Profile

- Profile Auto Selection

- Switch Profiles

- Configure TCP/IP

- Configuring Win XP

Security

- EAP-TLS

- EAP-TTLS

- PEAP (EAP-GTC)

- PEAP (EAP-MSCHAP V2)

- LEAP

- WPA Passphrase

Check Status or Diagnostics

- Check Current Status

- Check Driver Information

- Check Statistics

Connect to Another Network

Settings

- Signal Strength Display

- Data Display

- Display Refresh Interval

Tools

- Tray Icon

- Troubleshooting Utility

- Enable/ Disable the Radio

### Display Settings

To change the display settings, choose Options > Display Settings from the menu.

The display settings dialog box contains tools to set the:

Signal Strength Display Units | Sets the units used when displaying signal strength: percentage (%) or dBm.
Refresh Interval | Use the up/down arrows to set the display refresh interval in seconds.

Data Display

Sets the display to cumulative or relative:

- Relative displays the change in statistical data since the last update.
- Cumulative displays statistical data collected since opening the profile.