## Atheros Client Utility Help

Introduction

| System Requirements

Profile Management

| Create or Modify a Profile
| Remove a Profile
| Profile Auto Selection
| Switch Profiles
| Configure TCP/IP
| Configuring Win XP

Security

| EAP-TLS
| EAP-TTLS
| PEAP (EAP-GTC)
| PEAP (EAP-MSCHAP V2)
| LEAP
| WPA Passphrase

Check Status or Diagnostics

| Check Current Status
| Check Driver Information
| Check Statistics

Connect to Another Network

Settings

| Signal Strength Display
| Data Display
| Display Refresh Interval

Tools

| Tray Icon
| Troubleshooting Utility
| Enable/ Disable the Radio

### Ad Hoc Mode

In ad hoc mode, a wireless network adapter works within an independent basic service set (IBSS), as illustrated here. All stations communicate directly with other stations without using an access point (AP).

To connect to an ad hoc network, configure the profile for ad hoc mode.