## Atheros Client Utility Help

Introduction

- System Requirements

Profile Management

- Create or Modify a Profile

- Remove a Profile

- Profile Auto Selection

- Switch Profiles

- Configure TCP/IP

- Configuring Win XP

Security

- EAP-TLS

- EAP-TTLS

- PEAP (EAP-GTC)

- PEAP (EAP-MSCHAP V2)

- LEAP

- WPA Passphrase

Check Status or Diagnostics

- Check Current Status

- Check Driver Information

- Check Statistics

Connect to Another Network

Settings

- Signal Strength Display

- Data Display

- Display Refresh Interval

Tools

- Tray Icon

- Troubleshooting Utility

- Enable/ Disable the Radio

### Infrastructure (Access Point) Mode Profile Configuration

To configure a profile in infrastructure (access point) mode, change the Network Type in the Advanced tab. For access point mode, modify the settings:

- Transmit Power Level
- Power Save Mode
- 802.11b Preamble (if using 802.11b)
- Wireless Mode
- 802.11a Authentication Mode (if using 802.11a)

Make sure to also edit the General and Security tabs.