## Atheros Client Utility Help

Introduction

- System Requirements

Profile Management

- Create or Modify a Profile

- Remove a Profile

- Profile Auto Selection

- Switch Profiles

- Configure TCP/IP

- Configuring Win XP

Security

- EAP-TLS

- EAP-TTLS

- PEAP (EAP-GTC)

- PEAP (EAP-MSCHAP V2)

- LEAP

- WPA Passphrase

Check Status or Diagnostics

- Check Current Status

- Check Driver Information

- Check Statistics

Connect to Another Network

Settings

- Signal Strength Display

- Data Display

- Display Refresh Interval

Tools

- Tray Icon

- Troubleshooting Utility

- Enable/ Disable the Radio

### Troubleshooting Utility

The Troubleshooting Utility is an optional utility that identifies and resolves wireless adapter configuration and association problems when the adapter is in access point (infrastructure) mode.

This utility is available only in Mini PCI solutions.

To run the Troubleshooting Utility:

- From the Diagnostics tab, click the Troubleshooting button to run the Troubleshooting Utility.

- OR: Select Action > Troubleshooting from the action menu.

Click Run Test to run the troubleshooting utility tests:

- Driver Installation

- Card Insertion

- Card Enable

- Radio

- Association

- Authentication

- Network

The utility posts the test results as:

- Test passed: Successful test completion

- Test failed: The test failed because the wireless adapter is not configured improperly to associate to an access point

- Test bypassed: The test was not required for the active profile

To view a report of the tests, click View Report.

- To save the report, click Save Report and browse to the directory to save the report to.

> Name the file and click Save.

- Click Start Test to re-run the troubleshooting utility.