## Atheros Client Utility Help

Introduction

- System Requirements

Profile Management

- Create or Modify a Profile

- Remove a Profile

- Profile Auto Selection

- Switch Profiles

- Configure TCP/IP

- Configuring Win XP

Security

- EAP-TLS

- EAP-TTLS

- PEAP (EAP-GTC)

- PEAP (EAP-MSCHAP V2)

- LEAP

- WPA Passphrase

Check Status or Diagnostics

- Check Current Status

- Check Driver Information

- Check Statistics

Connect to Another Network

Settings

- Signal Strength Display

- Data Display

- Display Refresh Interval

Tools

- Tray Icon

- Troubleshooting Utility

- Enable/ Disable the Radio

### Switching to a different configuration profile

1. To switch to a different profile, go to the Profile Management tab.
2. Click on the profile name in the Profile List.
3. Click the Activate button.

The Profile List provides icons that specify the operational state for that profile. The list also provides icons that specify the signal strength for that profile.

See also Scan Available Networks.