;DrIvEr DeScRiPtIoN
;VeRsIoN = 2.11 Novell LAN Installation Information File for FETNWSRV
;CoPyRiGhT = (c) Copyright 2001 by VIA. All rights reserved.

VER: 2.11
SYN: 1.00

DR FETNWSRV
{
        DES:    $FETNWSRV_DES
        HELP:   $FETNWSRV_HELP
        PAR:    2.00                            ; Hardware Instance Number Aware
        PROD:   'PCI.1106.3043.*.*.*',          ; VT3043
                'PCI.1106.3065.*.*.*',          ; VT3065
                'PCI.1106.3106.*.*.*',          ; VT3106
                'PCI.1106.3053.*.*.*'           ; VT3053
                
        FILE:   FETNWSRV.LAN
        TIME:   20

        ;@#	CLIENT:	FETNWSRV.LAN
        ;@#	ALIAS:	FETNWSRV.LAN
        ;@# SPROD:  'VIA Technologies~VIA Rhine Family Fast Ethernet Adapter'

        PROMPT SLOT OPTIONAL
        {
                DES:    $FETNWSRV_SLOT_DES
                HELP:   $FETNWSRV_SLOT_HLP

                TYPE:   DECIMAL
                VAL:    1-65535
                DEF:    UNDEFINED
                OUT:    'SLOT=%s'
        }

        PR NODE
        {
        }

        FR FrameSelect
        {
                CH:     'Ethernet_802.3'
                CH:     'Ethernet_802.2'
                CH:     'Ethernet_SNAP'
                CH:     'Ethernet_II'
                DEF:    1,2                 ; Default flame type = 802.3, 802.2
        }

        ; We use LIST operation to instead of (2001/07/09), Ben
        ; ------------------------------------------\
        ;PR AUTO OPTIONAL
        ;{
        ;        DES:    $FETNWSRV_7
        ;        HELP:   $FETNWSRV_8
        ;
        ;        VAL:    0, 1
        ;        TYP:    HEX(1)
        ;        DEF:    UNDEFINED
        ;}

        ;PR FULLDUPLEX OPTIONAL
        ;{
        ;        DES:    $FETNWSRV_1
        ;        HELP:   $FETNWSRV_2
        ;
        ;        VAL:    0, 1
        ;        TYP:    HEX(1)
        ;        DEF:    UNDEFINED
        ;}
        
        ;PR SPEED OPTIONAL
        ;{
        ;        DES:    $FETNWSRV_11
        ;        HELP:   $FETNWSRV_12
        ;
        ;        VAL:    10, 100
        ;        TYPE:   DECIMAL
        ;        DEF:    UNDEFINED
        ;}
        ; ------------------------------------------/
        
        
        ; ---------------------------------------------------------
        ; LIST keywords [CONNECTIONTYPE]:
        ;   AUTOSENSE, 10BASET, 10BASETFD, 100BASETX, 100BASETXFD     
        ; ---------------------------------------------------------
        LI CONNECTIONTYPE OPT
        {
                DES:    $FETNWSRV_CONTYPE_DES
                HELP:   $FETNWSRV_CONTYPE_HLP

                CD:     $FETNWSRV_CAUTO_CD
                CH:     $FETNWSRV_CAUTO_CH
                CD:     $FETNWSRV_C10H_CD
                CH:     $FETNWSRV_C10H_CH
                CD:     $FETNWSRV_C10F_CD
                CH:     $FETNWSRV_C10F_CH
                CD:     $FETNWSRV_C100H_CD
                CH:     $FETNWSRV_C100H_CH
                CD:     $FETNWSRV_C100F_CD
                CH:     $FETNWSRV_C100F_CH
                DEF:    1                       ; DEFAULT=AUTOSENSE
                
                OUT:    'CONNECTIONTYPE=%s'     ; if use this, driver need to 
                                                ; support extra keyword routine for
                                                ; 'CONNECTIONTYPE'
        }
        
        ; ---------------------------------------------------------
        ; keywords [VID]:
        ;   0 ~ 4096
        ; ---------------------------------------------------------
        PROMPT VID OPTIONAL
        {
                DES:    $FETNWSRV_VID_DES
                HELP:   $FETNWSRV_VID_HLP

                TYPE:   DECIMAL
                VAL:    1-65535
                DEF:    UNDEFINED
                OUT:    'VID=%s'
        }
        
        ; --------------------------------------------------
        ; LIST keywords [FLOW_CONTROL]:
        ;   Enable, Disable, Hardware_default(or HD)
        ; --------------------------------------------------
        LI FLOW_CONTROL OPT
        {
                DES:    $FETNWSRV_FLOWCTL_DES
                HELP:   $FETNWSRV_FLOWCTL_HLP

                CD:     $FETNWSRV_FHD_CD
                CH:     $FETNWSRV_FHD_CH
                CD:     $FETNWSRV_FENA_CD
                CH:     $FETNWSRV_FENA_CH
                CD:     $FETNWSRV_FDIS_CD
                CH:     $FETNWSRV_FDIS_CH
                DEF:    1                       ; DEFAULT=Hardware_Default (HD)
                
                OUT:    'FLOW_CONTROL=%s'       ; if use this, driver need to 
                                                ; support extra keyword routine for
                                                ; 'FLOW_CONTROL'
        }
        
        ; --------------------------------------------------
        ; LIST keywords [TAG]:
        ;   Enable, Disable
        ; --------------------------------------------------
        LI TAG OPT
        {
                DES:    $FETNWSRV_TAG_DES
                HELP:   $FETNWSRV_TAG_HLP

                CD:     $FETNWSRV_TENA_CD
                CH:     $FETNWSRV_TENA_CH
                CD:     $FETNWSRV_TDIS_CD
                CH:     $FETNWSRV_TDIS_CH
                DEF:    2                       ; DEFAULT=Disable
                OUT:    'TAG=%s'                ; if use this, driver need to 
                                                ; support extra keyword routine for
                                                ; 'TAG'
                                                
                ;DES:    $FETNWSRV_PRI_DES
                ;HELP:   $FETNWSRV_PRI_HLP

                ;CD:     $FETNWSRV_PENA_CD
                ;CH:     $FETNWSRV_PENA_CH
                ;CD:     $FETNWSRV_PDIS_CD
                ;CH:     $FETNWSRV_PDIS_CH
                ;DEF:    2                       ; DEFAULT=Disable
                ;OUT:    'PRIORITY=%s'           ; if use this, driver need to 
                                                ; support extra keyword routine for
                                                ; 'PRIORITY'
        }
}


DLANG:  4
;English
        $FETNWSRV_DUPLEX_DES= "Full Duplex mode"
        $FETNWSRV_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $FETNWSRV_AUTO_DES  = "AUTO mode"
        $FETNWSRV_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $FETNWSRV_SPEED_DES = "SPEED selection"
        $FETNWSRV_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $FETNWSRV_SLOT_DES  = "Slot"
        $FETNWSRV_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $FETNWSRV_CONTYPE_DES   = "Media and Line Speed"
        $FETNWSRV_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_PRI_DES   = "Priority Transmit Support"
        $FETNWSRV_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"
                                        
        $FETNWSRV_TAG_DES   = "Tagging ability Support"
        $FETNWSRV_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                
        $FETNWSRV_FLOWCTL_DES   = "Flow control ability"
        $FETNWSRV_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_HCS_DES   = "Hardware Checksum Support"
        $FETNWSRV_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $FETNWSRV_VID_DES   = "VID number support for VLAN"
        $FETNWSRV_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $FETNWSRV_CAUTO_CD  = "Auto-Sense media type"
        $FETNWSRV_CAUTO_CH  = "Autosense"
        $FETNWSRV_C10H_CD   = "Twisted Pair 10MBPS"
        $FETNWSRV_C10H_CH   = "10BASET"
        $FETNWSRV_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $FETNWSRV_C10F_CH   = "10BASETFD"
        $FETNWSRV_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $FETNWSRV_C100H_CH  = "100BASETXFD"
        $FETNWSRV_C100F_CD  = "Fast Ethernet 100MBPS"
        $FETNWSRV_C100F_CH  = "100BASETX"
        

        $FETNWSRV_FHD_CD    = "Use Hardware Default"
        $FETNWSRV_FHD_CH    = "HD"
        $FETNWSRV_FENA_CD   = "Enable Flow Control"
        $FETNWSRV_FENA_CH   = "Enable"
        $FETNWSRV_FDIS_CD   = "Disable Flow Control"
        $FETNWSRV_FDIS_CH   = "Disable"
        
        $FETNWSRV_PENA_CD   = "Enable Priority Transmit"
        $FETNWSRV_PENA_CH   = "Enable"
        $FETNWSRV_PDIS_CD   = "Disable Priority Transmit"
        $FETNWSRV_PDIS_CH   = "Disable"
                                        
        $FETNWSRV_TENA_CD   = "Enable Tagging"
        $FETNWSRV_TENA_CH   = "Enable"
        $FETNWSRV_TDIS_CD   = "Disable Tagging"
        $FETNWSRV_TDIS_CH   = "Disable"
        
        $FETNWSRV_HENA_CD   = "Enable Hardware Checksum"
        $FETNWSRV_HENA_CH   = "Enable"
        $FETNWSRV_HDIS_CD   = "Disable Hardware Checksum"
        $FETNWSRV_HDIS_CH   = "Disable"

        $FETNWSRV_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $FETNWSRV_HELP      = "This driver (FETNWSRV.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

LANG:   6
;French
        $FETNWSRV_DUPLEX_DES= "Full Duplex mode"
        $FETNWSRV_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $FETNWSRV_AUTO_DES  = "AUTO mode"
        $FETNWSRV_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $FETNWSRV_SPEED_DES = "SPEED selection"
        $FETNWSRV_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $FETNWSRV_SLOT_DES  = "Slot"
        $FETNWSRV_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $FETNWSRV_CONTYPE_DES   = "Media and Line Speed"
        $FETNWSRV_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_PRI_DES   = "Priority Transmit Support"
        $FETNWSRV_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"
                                        
        $FETNWSRV_TAG_DES   = "Tagging ability Support"
        $FETNWSRV_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                
        $FETNWSRV_FLOWCTL_DES   = "Flow control ability"
        $FETNWSRV_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_HCS_DES   = "Hardware Checksum Support"
        $FETNWSRV_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $FETNWSRV_VID_DES   = "VID number support for VLAN"
        $FETNWSRV_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $FETNWSRV_CAUTO_CD  = "Auto-Sense media type"
        $FETNWSRV_CAUTO_CH  = "Autosense"
        $FETNWSRV_C10H_CD   = "Twisted Pair 10MBPS"
        $FETNWSRV_C10H_CH   = "10BASET"
        $FETNWSRV_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $FETNWSRV_C10F_CH   = "10BASETFD"
        $FETNWSRV_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $FETNWSRV_C100H_CH  = "100BASETXFD"
        $FETNWSRV_C100F_CD  = "Fast Ethernet 100MBPS"
        $FETNWSRV_C100F_CH  = "100BASETX"
        

        $FETNWSRV_FHD_CD    = "Use Hardware Default"
        $FETNWSRV_FHD_CH    = "HD"
        $FETNWSRV_FENA_CD   = "Enable Flow Control"
        $FETNWSRV_FENA_CH   = "Enable"
        $FETNWSRV_FDIS_CD   = "Disable Flow Control"
        $FETNWSRV_FDIS_CH   = "Disable"
        
        
        $FETNWSRV_PENA_CD   = "Enable Priority Transmit"
        $FETNWSRV_PENA_CH   = "Enable"
        $FETNWSRV_PDIS_CD   = "Disable Priority Transmit"
        $FETNWSRV_PDIS_CH   = "Disable"

        $FETNWSRV_TENA_CD   = "Enable Tagging"
        $FETNWSRV_TENA_CH   = "Enable"
        $FETNWSRV_TDIS_CD   = "Disable Tagging"
        $FETNWSRV_TDIS_CH   = "Disable"
        
        $FETNWSRV_HENA_CD   = "Enable Hardware Checksum"
        $FETNWSRV_HENA_CH   = "Enable"
        $FETNWSRV_HDIS_CD   = "Disable Hardware Checksum"
        $FETNWSRV_HDIS_CH   = "Disable"

        $FETNWSRV_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $FETNWSRV_HELP      = "This driver (FETNWSRV.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."
LANG:   7
;German
        $FETNWSRV_DUPLEX_DES= "Full Duplex mode"
        $FETNWSRV_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $FETNWSRV_AUTO_DES  = "AUTO mode"
        $FETNWSRV_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $FETNWSRV_SPEED_DES = "SPEED selection"
        $FETNWSRV_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $FETNWSRV_SLOT_DES  = "Slot"
        $FETNWSRV_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $FETNWSRV_CONTYPE_DES   = "Media and Line Speed"
        $FETNWSRV_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_PRI_DES   = "Priority Transmit Support"
        $FETNWSRV_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"

        $FETNWSRV_TAG_DES   = "Tagging ability Support"
        $FETNWSRV_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                        
        $FETNWSRV_FLOWCTL_DES   = "Flow control ability"
        $FETNWSRV_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_HCS_DES   = "Hardware Checksum Support"
        $FETNWSRV_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $FETNWSRV_VID_DES   = "VID number support for VLAN"
        $FETNWSRV_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $FETNWSRV_CAUTO_CD  = "Auto-Sense media type"
        $FETNWSRV_CAUTO_CH  = "Autosense"
        $FETNWSRV_C10H_CD   = "Twisted Pair 10MBPS"
        $FETNWSRV_C10H_CH   = "10BASET"
        $FETNWSRV_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $FETNWSRV_C10F_CH   = "10BASETFD"
        $FETNWSRV_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $FETNWSRV_C100H_CH  = "100BASETXFD"
        $FETNWSRV_C100F_CD  = "Fast Ethernet 100MBPS"
        $FETNWSRV_C100F_CH  = "100BASETX"
        

        $FETNWSRV_FHD_CD    = "Use Hardware Default"
        $FETNWSRV_FHD_CH    = "HD"
        $FETNWSRV_FENA_CD   = "Enable Flow Control"
        $FETNWSRV_FENA_CH   = "Enable"
        $FETNWSRV_FDIS_CD   = "Disable Flow Control"
        $FETNWSRV_FDIS_CH   = "Disable"
        
        
        $FETNWSRV_PENA_CD   = "Enable Priority Transmit"
        $FETNWSRV_PENA_CH   = "Enable"
        $FETNWSRV_PDIS_CD   = "Disable Priority Transmit"
        $FETNWSRV_PDIS_CH   = "Disable"
                                        
        $FETNWSRV_TENA_CD   = "Enable Tagging"
        $FETNWSRV_TENA_CH   = "Enable"
        $FETNWSRV_TDIS_CD   = "Disable Tagging"
        $FETNWSRV_TDIS_CH   = "Disable"
        
        $FETNWSRV_HENA_CD   = "Enable Hardware Checksum"
        $FETNWSRV_HENA_CH   = "Enable"
        $FETNWSRV_HDIS_CD   = "Disable Hardware Checksum"
        $FETNWSRV_HDIS_CH   = "Disable"

        $FETNWSRV_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $FETNWSRV_HELP      = "This driver (FETNWSRV.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

LANG:   8
;Italian
        $FETNWSRV_DUPLEX_DES= "Full Duplex mode"
        $FETNWSRV_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $FETNWSRV_AUTO_DES  = "AUTO mode"
        $FETNWSRV_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $FETNWSRV_SPEED_DES = "SPEED selection"
        $FETNWSRV_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $FETNWSRV_SLOT_DES  = "Slot"
        $FETNWSRV_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $FETNWSRV_CONTYPE_DES   = "Media and Line Speed"
        $FETNWSRV_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_PRI_DES   = "Priority Transmit Support"
        $FETNWSRV_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"

        $FETNWSRV_TAG_DES   = "Tagging ability Support"
        $FETNWSRV_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                        
        $FETNWSRV_FLOWCTL_DES   = "Flow control ability"
        $FETNWSRV_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_HCS_DES   = "Hardware Checksum Support"
        $FETNWSRV_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $FETNWSRV_VID_DES   = "VID number support for VLAN"
        $FETNWSRV_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $FETNWSRV_CAUTO_CD  = "Auto-Sense media type"
        $FETNWSRV_CAUTO_CH  = "Autosense"
        $FETNWSRV_C10H_CD   = "Twisted Pair 10MBPS"
        $FETNWSRV_C10H_CH   = "10BASET"
        $FETNWSRV_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $FETNWSRV_C10F_CH   = "10BASETFD"
        $FETNWSRV_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $FETNWSRV_C100H_CH  = "100BASETXFD"
        $FETNWSRV_C100F_CD  = "Fast Ethernet 100MBPS"
        $FETNWSRV_C100F_CH  = "100BASETX"
        

        $FETNWSRV_FHD_CD    = "Use Hardware Default"
        $FETNWSRV_FHD_CH    = "HD"
        $FETNWSRV_FENA_CD   = "Enable Flow Control"
        $FETNWSRV_FENA_CH   = "Enable"
        $FETNWSRV_FDIS_CD   = "Disable Flow Control"
        $FETNWSRV_FDIS_CH   = "Disable"
        
        
        $FETNWSRV_PENA_CD   = "Enable Priority Transmit"
        $FETNWSRV_PENA_CH   = "Enable"
        $FETNWSRV_PDIS_CD   = "Disable Priority Transmit"
        $FETNWSRV_PDIS_CH   = "Disable"
                                        
        $FETNWSRV_TENA_CD   = "Enable Tagging"
        $FETNWSRV_TENA_CH   = "Enable"
        $FETNWSRV_TDIS_CD   = "Disable Tagging"
        $FETNWSRV_TDIS_CH   = "Disable"
        
        $FETNWSRV_HENA_CD   = "Enable Hardware Checksum"
        $FETNWSRV_HENA_CH   = "Enable"
        $FETNWSRV_HDIS_CD   = "Disable Hardware Checksum"
        $FETNWSRV_HDIS_CH   = "Disable"

        $FETNWSRV_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $FETNWSRV_HELP      = "This driver (FETNWSRV.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

LANG:   14
;Spanish
        $FETNWSRV_DUPLEX_DES= "Full Duplex mode"
        $FETNWSRV_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $FETNWSRV_AUTO_DES  = "AUTO mode"
        $FETNWSRV_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $FETNWSRV_SPEED_DES = "SPEED selection"
        $FETNWSRV_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $FETNWSRV_SLOT_DES  = "Slot"
        $FETNWSRV_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $FETNWSRV_CONTYPE_DES   = "Media and Line Speed"
        $FETNWSRV_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_PRI_DES   = "Priority Transmit Support"
        $FETNWSRV_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"

        $FETNWSRV_TAG_DES   = "Tagging ability Support"
        $FETNWSRV_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                        
        $FETNWSRV_FLOWCTL_DES   = "Flow control ability"
        $FETNWSRV_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_HCS_DES   = "Hardware Checksum Support"
        $FETNWSRV_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $FETNWSRV_VID_DES   = "VID number support for VLAN"
        $FETNWSRV_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $FETNWSRV_CAUTO_CD  = "Auto-Sense media type"
        $FETNWSRV_CAUTO_CH  = "Autosense"
        $FETNWSRV_C10H_CD   = "Twisted Pair 10MBPS"
        $FETNWSRV_C10H_CH   = "10BASET"
        $FETNWSRV_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $FETNWSRV_C10F_CH   = "10BASETFD"
        $FETNWSRV_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $FETNWSRV_C100H_CH  = "100BASETXFD"
        $FETNWSRV_C100F_CD  = "Fast Ethernet 100MBPS"
        $FETNWSRV_C100F_CH  = "100BASETX"
        

        $FETNWSRV_FHD_CD    = "Use Hardware Default"
        $FETNWSRV_FHD_CH    = "HD"
        $FETNWSRV_FENA_CD   = "Enable Flow Control"
        $FETNWSRV_FENA_CH   = "Enable"
        $FETNWSRV_FDIS_CD   = "Disable Flow Control"
        $FETNWSRV_FDIS_CH   = "Disable"
        
        
        $FETNWSRV_PENA_CD   = "Enable Priority Transmit"
        $FETNWSRV_PENA_CH   = "Enable"
        $FETNWSRV_PDIS_CD   = "Disable Priority Transmit"
        $FETNWSRV_PDIS_CH   = "Disable"
                                        
        $FETNWSRV_TENA_CD   = "Enable Tagging"
        $FETNWSRV_TENA_CH   = "Enable"
        $FETNWSRV_TDIS_CD   = "Disable Tagging"
        $FETNWSRV_TDIS_CH   = "Disable"
        
        $FETNWSRV_HENA_CD   = "Enable Hardware Checksum"
        $FETNWSRV_HENA_CH   = "Enable"
        $FETNWSRV_HDIS_CD   = "Disable Hardware Checksum"
        $FETNWSRV_HDIS_CH   = "Disable"

        $FETNWSRV_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $FETNWSRV_HELP      = "This driver (FETNWSRV.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

LANG:   9
;Japanese
        $FETNWSRV_DUPLEX_DES= "Full Duplex mode"
        $FETNWSRV_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $FETNWSRV_AUTO_DES  = "AUTO mode"
        $FETNWSRV_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $FETNWSRV_SPEED_DES = "SPEED selection"
        $FETNWSRV_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $FETNWSRV_SLOT_DES  = "Slot"
        $FETNWSRV_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $FETNWSRV_CONTYPE_DES   = "Media and Line Speed"
        $FETNWSRV_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_PRI_DES   = "Priority Transmit Support"
        $FETNWSRV_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"

        $FETNWSRV_TAG_DES   = "Tagging ability Support"
        $FETNWSRV_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                        
        $FETNWSRV_FLOWCTL_DES   = "Flow control ability"
        $FETNWSRV_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_HCS_DES   = "Hardware Checksum Support"
        $FETNWSRV_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $FETNWSRV_VID_DES   = "VID number support for VLAN"
        $FETNWSRV_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $FETNWSRV_CAUTO_CD  = "Auto-Sense media type"
        $FETNWSRV_CAUTO_CH  = "Autosense"
        $FETNWSRV_C10H_CD   = "Twisted Pair 10MBPS"
        $FETNWSRV_C10H_CH   = "10BASET"
        $FETNWSRV_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $FETNWSRV_C10F_CH   = "10BASETFD"
        $FETNWSRV_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $FETNWSRV_C100H_CH  = "100BASETXFD"
        $FETNWSRV_C100F_CD  = "Fast Ethernet 100MBPS"
        $FETNWSRV_C100F_CH  = "100BASETX"
        

        $FETNWSRV_FHD_CD    = "Use Hardware Default"
        $FETNWSRV_FHD_CH    = "HD"
        $FETNWSRV_FENA_CD   = "Enable Flow Control"
        $FETNWSRV_FENA_CH   = "Enable"
        $FETNWSRV_FDIS_CD   = "Disable Flow Control"
        $FETNWSRV_FDIS_CH   = "Disable"
        
        
        $FETNWSRV_PENA_CD   = "Enable Priority Transmit"
        $FETNWSRV_PENA_CH   = "Enable"
        $FETNWSRV_PDIS_CD   = "Disable Priority Transmit"
        $FETNWSRV_PDIS_CH   = "Disable"
                                        
        $FETNWSRV_TENA_CD   = "Enable Tagging"
        $FETNWSRV_TENA_CH   = "Enable"
        $FETNWSRV_TDIS_CD   = "Disable Tagging"
        $FETNWSRV_TDIS_CH   = "Disable"
        
        $FETNWSRV_HENA_CD   = "Enable Hardware Checksum"
        $FETNWSRV_HENA_CH   = "Enable"
        $FETNWSRV_HDIS_CD   = "Disable Hardware Checksum"
        $FETNWSRV_HDIS_CH   = "Disable"

        $FETNWSRV_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $FETNWSRV_HELP      = "This driver (FETNWSRV.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

LANG:   10
;Korean
        $FETNWSRV_DUPLEX_DES= "Full Duplex mode"
        $FETNWSRV_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $FETNWSRV_AUTO_DES  = "AUTO mode"
        $FETNWSRV_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $FETNWSRV_SPEED_DES = "SPEED selection"
        $FETNWSRV_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $FETNWSRV_SLOT_DES  = "Slot"
        $FETNWSRV_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $FETNWSRV_CONTYPE_DES   = "Media and Line Speed"
        $FETNWSRV_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."

        $FETNWSRV_PRI_DES   = "Priority Transmit Support"
        $FETNWSRV_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"

        $FETNWSRV_TAG_DES   = "Tagging ability Support"
        $FETNWSRV_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                       
        $FETNWSRV_FLOWCTL_DES   = "Flow control ability"
        $FETNWSRV_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_HCS_DES   = "Hardware Checksum Support"
        $FETNWSRV_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $FETNWSRV_VID_DES   = "VID number support for VLAN"
        $FETNWSRV_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $FETNWSRV_CAUTO_CD  = "Auto-Sense media type"
        $FETNWSRV_CAUTO_CH  = "Autosense"
        $FETNWSRV_C10H_CD   = "Twisted Pair 10MBPS"
        $FETNWSRV_C10H_CH   = "10BASET"
        $FETNWSRV_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $FETNWSRV_C10F_CH   = "10BASETFD"
        $FETNWSRV_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $FETNWSRV_C100H_CH  = "100BASETXFD"
        $FETNWSRV_C100F_CD  = "Fast Ethernet 100MBPS"
        $FETNWSRV_C100F_CH  = "100BASETX"
        

        $FETNWSRV_FHD_CD    = "Use Hardware Default"
        $FETNWSRV_FHD_CH    = "HD"
        $FETNWSRV_FENA_CD   = "Enable Flow Control"
        $FETNWSRV_FENA_CH   = "Enable"
        $FETNWSRV_FDIS_CD   = "Disable Flow Control"
        $FETNWSRV_FDIS_CH   = "Disable"
        
        
        $FETNWSRV_PENA_CD   = "Enable Priority Transmit"
        $FETNWSRV_PENA_CH   = "Enable"
        $FETNWSRV_PDIS_CD   = "Disable Priority Transmit"
        $FETNWSRV_PDIS_CH   = "Disable"
                                        
        $FETNWSRV_TENA_CD   = "Enable Tagging"
        $FETNWSRV_TENA_CH   = "Enable"
        $FETNWSRV_TDIS_CD   = "Disable Tagging"
        $FETNWSRV_TDIS_CH   = "Disable"
        
        $FETNWSRV_HENA_CD   = "Enable Hardware Checksum"
        $FETNWSRV_HENA_CH   = "Enable"
        $FETNWSRV_HDIS_CD   = "Disable Hardware Checksum"
        $FETNWSRV_HDIS_CH   = "Disable"

        $FETNWSRV_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $FETNWSRV_HELP      = "This driver (FETNWSRV.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

LANG:   12
;Portugese (Brazil)
        $FETNWSRV_DUPLEX_DES= "Full Duplex mode"
        $FETNWSRV_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $FETNWSRV_AUTO_DES  = "AUTO mode"
        $FETNWSRV_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $FETNWSRV_SPEED_DES = "SPEED selection"
        $FETNWSRV_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $FETNWSRV_SLOT_DES  = "Slot"
        $FETNWSRV_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $FETNWSRV_CONTYPE_DES   = "Media and Line Speed"
        $FETNWSRV_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_PRI_DES   = "Priority Transmit Support"
        $FETNWSRV_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"

        $FETNWSRV_TAG_DES   = "Tagging ability Support"
        $FETNWSRV_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                        
        $FETNWSRV_FLOWCTL_DES   = "Flow control ability"
        $FETNWSRV_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_HCS_DES   = "Hardware Checksum Support"
        $FETNWSRV_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $FETNWSRV_VID_DES   = "VID number support for VLAN"
        $FETNWSRV_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $FETNWSRV_CAUTO_CD  = "Auto-Sense media type"
        $FETNWSRV_CAUTO_CH  = "Autosense"
        $FETNWSRV_C10H_CD   = "Twisted Pair 10MBPS"
        $FETNWSRV_C10H_CH   = "10BASET"
        $FETNWSRV_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $FETNWSRV_C10F_CH   = "10BASETFD"
        $FETNWSRV_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $FETNWSRV_C100H_CH  = "100BASETXFD"
        $FETNWSRV_C100F_CD  = "Fast Ethernet 100MBPS"
        $FETNWSRV_C100F_CH  = "100BASETX"
        

        $FETNWSRV_FHD_CD    = "Use Hardware Default"
        $FETNWSRV_FHD_CH    = "HD"
        $FETNWSRV_FENA_CD   = "Enable Flow Control"
        $FETNWSRV_FENA_CH   = "Enable"
        $FETNWSRV_FDIS_CD   = "Disable Flow Control"
        $FETNWSRV_FDIS_CH   = "Disable"
        
        
        $FETNWSRV_PENA_CD   = "Enable Priority Transmit"
        $FETNWSRV_PENA_CH   = "Enable"
        $FETNWSRV_PDIS_CD   = "Disable Priority Transmit"
        $FETNWSRV_PDIS_CH   = "Disable"
                                        
        $FETNWSRV_TENA_CD   = "Enable Tagging"
        $FETNWSRV_TENA_CH   = "Enable"
        $FETNWSRV_TDIS_CD   = "Disable Tagging"
        $FETNWSRV_TDIS_CH   = "Disable"
        
        $FETNWSRV_HENA_CD   = "Enable Hardware Checksum"
        $FETNWSRV_HENA_CH   = "Enable"
        $FETNWSRV_HDIS_CD   = "Disable Hardware Checksum"
        $FETNWSRV_HDIS_CH   = "Disable"

        $FETNWSRV_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $FETNWSRV_HELP      = "This driver (FETNWSRV.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

LANG:   13
;Russian
        $FETNWSRV_DUPLEX_DES= "Full Duplex mode"
        $FETNWSRV_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $FETNWSRV_AUTO_DES  = "AUTO mode"
        $FETNWSRV_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $FETNWSRV_SPEED_DES = "SPEED selection"
        $FETNWSRV_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $FETNWSRV_SLOT_DES  = "Slot"
        $FETNWSRV_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $FETNWSRV_CONTYPE_DES   = "Media and Line Speed"
        $FETNWSRV_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_PRI_DES   = "Priority Transmit Support"
        $FETNWSRV_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"

        $FETNWSRV_TAG_DES   = "Tagging ability Support"
        $FETNWSRV_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                        
        $FETNWSRV_FLOWCTL_DES   = "Flow control ability"
        $FETNWSRV_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_HCS_DES   = "Hardware Checksum Support"
        $FETNWSRV_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $FETNWSRV_VID_DES   = "VID number support for VLAN"
        $FETNWSRV_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $FETNWSRV_CAUTO_CD  = "Auto-Sense media type"
        $FETNWSRV_CAUTO_CH  = "Autosense"
        $FETNWSRV_C10H_CD   = "Twisted Pair 10MBPS"
        $FETNWSRV_C10H_CH   = "10BASET"
        $FETNWSRV_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $FETNWSRV_C10F_CH   = "10BASETFD"
        $FETNWSRV_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $FETNWSRV_C100H_CH  = "100BASETXFD"
        $FETNWSRV_C100F_CD  = "Fast Ethernet 100MBPS"
        $FETNWSRV_C100F_CH  = "100BASETX"
        

        $FETNWSRV_FHD_CD    = "Use Hardware Default"
        $FETNWSRV_FHD_CH    = "HD"
        $FETNWSRV_FENA_CD   = "Enable Flow Control"
        $FETNWSRV_FENA_CH   = "Enable"
        $FETNWSRV_FDIS_CD   = "Disable Flow Control"
        $FETNWSRV_FDIS_CH   = "Disable"
        
        
        $FETNWSRV_PENA_CD   = "Enable Priority Transmit"
        $FETNWSRV_PENA_CH   = "Enable"
        $FETNWSRV_PDIS_CD   = "Disable Priority Transmit"
        $FETNWSRV_PDIS_CH   = "Disable"
                                        
        $FETNWSRV_TENA_CD   = "Enable Tagging"
        $FETNWSRV_TENA_CH   = "Enable"
        $FETNWSRV_TDIS_CD   = "Disable Tagging"
        $FETNWSRV_TDIS_CH   = "Disable"
        
        $FETNWSRV_HENA_CD   = "Enable Hardware Checksum"
        $FETNWSRV_HENA_CH   = "Enable"
        $FETNWSRV_HDIS_CD   = "Disable Hardware Checksum"
        $FETNWSRV_HDIS_CH   = "Disable"

        $FETNWSRV_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $FETNWSRV_HELP      = "This driver (FETNWSRV.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

LANG:   16
;Chinese (Traditional)
        $FETNWSRV_DUPLEX_DES= "Full Duplex mode"
        $FETNWSRV_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $FETNWSRV_AUTO_DES  = "AUTO mode"
        $FETNWSRV_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $FETNWSRV_SPEED_DES = "SPEED selection"
        $FETNWSRV_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $FETNWSRV_SLOT_DES  = "Slot"
        $FETNWSRV_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $FETNWSRV_CONTYPE_DES   = "Media and Line Speed"
        $FETNWSRV_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_PRI_DES   = "Priority Transmit Support"
        $FETNWSRV_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"

        $FETNWSRV_TAG_DES   = "Tagging ability Support"
        $FETNWSRV_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                        
        $FETNWSRV_FLOWCTL_DES   = "Flow control ability"
        $FETNWSRV_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_HCS_DES   = "Hardware Checksum Support"
        $FETNWSRV_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $FETNWSRV_VID_DES   = "VID number support for VLAN"
        $FETNWSRV_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $FETNWSRV_CAUTO_CD  = "Auto-Sense media type"
        $FETNWSRV_CAUTO_CH  = "Autosense"
        $FETNWSRV_C10H_CD   = "Twisted Pair 10MBPS"
        $FETNWSRV_C10H_CH   = "10BASET"
        $FETNWSRV_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $FETNWSRV_C10F_CH   = "10BASETFD"
        $FETNWSRV_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $FETNWSRV_C100H_CH  = "100BASETXFD"
        $FETNWSRV_C100F_CD  = "Fast Ethernet 100MBPS"
        $FETNWSRV_C100F_CH  = "100BASETX"
        

        $FETNWSRV_FHD_CD    = "Use Hardware Default"
        $FETNWSRV_FHD_CH    = "HD"
        $FETNWSRV_FENA_CD   = "Enable Flow Control"
        $FETNWSRV_FENA_CH   = "Enable"
        $FETNWSRV_FDIS_CD   = "Disable Flow Control"
        $FETNWSRV_FDIS_CH   = "Disable"
        
        
        $FETNWSRV_PENA_CD   = "Enable Priority Transmit"
        $FETNWSRV_PENA_CH   = "Enable"
        $FETNWSRV_PDIS_CD   = "Disable Priority Transmit"
        $FETNWSRV_PDIS_CH   = "Disable"
                                        
        $FETNWSRV_TENA_CD   = "Enable Tagging"
        $FETNWSRV_TENA_CH   = "Enable"
        $FETNWSRV_TDIS_CD   = "Disable Tagging"
        $FETNWSRV_TDIS_CH   = "Disable"
        
        $FETNWSRV_HENA_CD   = "Enable Hardware Checksum"
        $FETNWSRV_HENA_CH   = "Enable"
        $FETNWSRV_HDIS_CD   = "Disable Hardware Checksum"
        $FETNWSRV_HDIS_CH   = "Disable"

        $FETNWSRV_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $FETNWSRV_HELP      = "This driver (FETNWSRV.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

LANG:   1
;Chinese (Simplified)
        $FETNWSRV_DUPLEX_DES= "Full Duplex mode"
        $FETNWSRV_DUPLEX_HLP= "Enable the Full Duplex Function."
        
        $FETNWSRV_AUTO_DES  = "AUTO mode"
        $FETNWSRV_AUTO_HLP  = "Enable the AUTO Negotiation Function."
        
        $FETNWSRV_SPEED_DES = "SPEED selection"
        $FETNWSRV_SPEED_HLP = "Select the SPEED between 10 and 100."
        
        $FETNWSRV_SLOT_DES  = "Slot"
        $FETNWSRV_SLOT_HLP  = "Enter the PCI Slot number of your LAN card
                               to enable PCI auto config function."

        $FETNWSRV_CONTYPE_DES   = "Media and Line Speed"
        $FETNWSRV_CONTYPE_HLP   = "Choose the connection/media type you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_PRI_DES   = "Priority Transmit Support"
        $FETNWSRV_PRI_HLP   = "Choose the priority transmit function you would
                                like to use, or NONE for preprogramed card's
                                default"

        $FETNWSRV_TAG_DES   = "Tagging ability Support"
        $FETNWSRV_TAG_HLP   = "Choose the tagging function you would like to use, 
                                or NONE for preprogramed card's default"
                                        
        $FETNWSRV_FLOWCTL_DES   = "Flow control ability"
        $FETNWSRV_FLOWCTL_HLP   = "Choose the flow control ability you would
                                    like to use, or NONE for preprogramed card's
                                    default."
        
        $FETNWSRV_HCS_DES   = "Hardware Checksum Support"
        $FETNWSRV_HCS_HLP   = "Choose the hardware checksum function you would
                                like to use, or NONE for preprogramed card's
                                default"
        
        $FETNWSRV_VID_DES   = "VID number support for VLAN"
        $FETNWSRV_VID_HLP   = "Enter the VID number of your LAN card
                                to support VLAN function."
                                        
        $FETNWSRV_CAUTO_CD  = "Auto-Sense media type"
        $FETNWSRV_CAUTO_CH  = "Autosense"
        $FETNWSRV_C10H_CD   = "Twisted Pair 10MBPS"
        $FETNWSRV_C10H_CH   = "10BASET"
        $FETNWSRV_C10F_CD   = "Twisted pair - Full Duplex 10MBPS"
        $FETNWSRV_C10F_CH   = "10BASETFD"
        $FETNWSRV_C100H_CD  = "Twisted pair - Full Duplex 100MBPS"
        $FETNWSRV_C100H_CH  = "100BASETXFD"
        $FETNWSRV_C100F_CD  = "Fast Ethernet 100MBPS"
        $FETNWSRV_C100F_CH  = "100BASETX"
        

        $FETNWSRV_FHD_CD    = "Use Hardware Default"
        $FETNWSRV_FHD_CH    = "HD"
        $FETNWSRV_FENA_CD   = "Enable Flow Control"
        $FETNWSRV_FENA_CH   = "Enable"
        $FETNWSRV_FDIS_CD   = "Disable Flow Control"
        $FETNWSRV_FDIS_CH   = "Disable"
        
        
        $FETNWSRV_PENA_CD   = "Enable Priority Transmit"
        $FETNWSRV_PENA_CH   = "Enable"
        $FETNWSRV_PDIS_CD   = "Disable Priority Transmit"
        $FETNWSRV_PDIS_CH   = "Disable"
                                        
        $FETNWSRV_TENA_CD   = "Enable Tagging"
        $FETNWSRV_TENA_CH   = "Enable"
        $FETNWSRV_TDIS_CD   = "Disable Tagging"
        $FETNWSRV_TDIS_CH   = "Disable"
        
        $FETNWSRV_HENA_CD   = "Enable Hardware Checksum"
        $FETNWSRV_HENA_CH   = "Enable"
        $FETNWSRV_HDIS_CD   = "Disable Hardware Checksum"
        $FETNWSRV_HDIS_CH   = "Disable"

        $FETNWSRV_DES       = "VIA Rhine Family Fast Ethernet Adapter"
        $FETNWSRV_HELP      = "This driver (FETNWSRV.LAN) supports PCI Fast Ethernet
                                network boards installed in PCI expansion slots in
                                server. You can install up to four boards as
                                long as their settings do not conflict."

;DrIvEr DeScRiPtIoN EnD
