#
# format for txtsetup.oem.
#
# General format:
#
# [section]
# key = value1,value2,...
#
#
# The hash ('#') introduces a comment.
# Strings with embedded spaces, commas, or hashes should be double-quoted
#


# This section lists all disks in the disk set.
#
# <description> is a descriptive name for a disk, used when
#   prompting for the disk
# <tagfile> is a file whose presence allows setup to recognize
#   that the disk is inserted.
# <directory> is where the files are located on the disk.
#

[Disks]
d1 = "VIA Serial ATA RAID Controller Driver ", \VT8237, \winxp
d2 = "VIA Serial ATA RAID Controller Driver ", \VT8237, \win2000
d3 = "VIA Serial ATA RAID Controller Driver ", \VT8237, \winnt40
d4 = "VIA Serial ATA RAID Controller Driver ", \VT8237, \2003ia32


# This section lists the default selection for each 'required'
# hardware component.  If a line is not present for a component,
# the default defaults to the first item in the [<component_name>]
# section (see below).
#
# <component_name> is one of computer, display, keyboard, mouse, scsi
# <id> is a unique <within the component> string to be associated
#   with an option.

[Defaults]

scsi = VIARAID_VT3149_XP



# This section lists the options available for a particular component.
#
# <id> is the unique string for the option
# <description> is a text string, presented to the user in a menu
# <key_name> gives the name of the key to be created for the component in
#   HKEY_LOCAL_MACHINE\ControlSet001\Services

[scsi]
VIARAID_VT3149_2003IA32 = "VIA Serial ATA RAID Controller(Windows 2003 IA32)",VT8237
VIARAID_VT3149_XP = "VIA Serial ATA RAID Controller(Windows XP)",VT8237
VIARAID_VT3149_2K = "VIA Serial ATA RAID Controller(Windows 2000)",VT8237
VIARAID_VT3149_NT = "VIA Serial ATA RAID Controller(Windows NT4)",VT8237


# This section lists the files that should be copied if the user
# selects a particular component option.
#
# <file_type> is one of driver, port, class, dll, hal, inf, or detect.
#   See below.
# <source_disk> identifies where the file is to be copied from, and must
#   match en entry in the [Disks] section.
# <filename> is the name of the file. This will be appended to the
#   directory specified for the disk in the [Disks] section to form the
#   full path of the file on the disk.
#=======================================#
[Files.scsi.VIARAID_VT3149_2003IA32]
driver = d4, viasraid.sys, viasraid
inf = d4, viasraid.inf
## Cat file directive. It should be marked with non-digital signed driver
catalog = d4, viasraid.cat

[Files.scsi.VIARAID_VT3149_XP]
driver = d1, viasraid.sys, viasraid
#dll = d1, setupvia.dll
inf = d1, viasraid.inf
## Cat file directive. It should be marked with non-digital signed driver
catalog = d1, viasraid.cat

[Files.scsi.VIARAID_VT3149_2K]
driver = d2, viasraid.sys, viasraid
#dll = d2, setupvia.dll
inf = d2, viasraid.inf
## Cat file directive. It should be marked with non-digital signed driver
catalog = d2, viasraid.cat

[Files.scsi.VIARAID_VT3149_NT]
driver = d3, viasraid.sys, viasraid
inf = d3, viasraid.inf

[HardwareIds.scsi.VIARAID_VT3149_2003IA32]
id = "PCI\VEN_1106&DEV_3149","viasraid"

[HardwareIds.scsi.VIARAID_VT3149_XP]
id = "PCI\VEN_1106&DEV_3149","viasraid"

[HardwareIds.scsi.VIARAID_VT3149_2K]
id = "PCI\VEN_1106&DEV_3149","viasraid"



# This section specifies values to be set in the registry for
# particular component options.  Required values in the services\xxx
# key are created automatically -- use this section to specify additional
# keys to be created in services\xxx and values in services\xxx and
# services\xxx\yyy.
#
# <key_name> is relative to the services node for this device.
#   If it is empty, then it refers to the services node.
#   If specified, the key is created first.
# <value_name> specifies the value to be set within the key
# <value_type> is a string like REG_DWORD.  See below.
# <value> specifies the actual value; its format depends on <value_type>

[Config.VT6420]

value = "", Tag, REG_DWORD, 1
#HP-Delete following line
#value = "Parameters\PnpInterface", 5, REG_DWORD, 1
