;==========================================================================;
; Name:	LVTV.INF
; Purpose:	INF for LifeView TV Card Win9x/2K/XP Drivers
; Author:	Robin Zhang
; Modified by : Pink
;
; Copyright (c) 2002-2003 Animation Technologies Inc.
; All Rights Reserved.
;
;==========================================================================;
[Version]
LayoutFile	= Layout.inf, Layout1.inf, Layout2.inf
signature	= "$CHICAGO$"
Class		= Media
ClassGUID	= {4d36e96c-e325-11ce-bfc1-08002be10318}
Provider	= %Lifeview%
CatalogFile	= lifeview.cat
DriverVer	= 09/22/2004, 2.3.0.235

[Manufacturer]
%Lifeview%	= Lifeview

[DestinationDirs]
LVCap138.CopyDrivers	= 10, system32\drivers
LVTuner.CopyDrivers	= 10, system32\drivers
Phi713x.CopyFiles	= 11

[SourceDisksNames]
1 = %Disk1%,,

[ControlFlags]
ExcludeFromSelect	=*

[SourceDisksFiles]
lvcap138.sys	= 1
lvtuner.sys	= 1

34pciurd.dll	= 1
34i2curd.dll	= 1
34api.dll	= 1
34dd.dll	= 1
34ds.dll	= 1
34dialog.dll	= 1
34dlg2.dll	= 1
34TvCtrl.dll	= 1
34com.dll	= 1
Prop7134.dll	= 1

;kstvtune.ax		= 1, win9x 
;[SourceDisksFiles.x86]
;kstvtune.ax		= 1, winnt


[Lifeview]
%Fly2100.DeviceDesc%	= LVCap138E.Device,  PCI\VEN_1131&DEV_7130&SUBSYS_01365168
%FlyDV2000.DeviceDesc%	= LVCap138E.Device,  PCI\VEN_1131&DEV_7130&SUBSYS_01375168
%Fly2000.DeviceDesc%	= LVCap138E.Device,  PCI\VEN_1131&DEV_7130&SUBSYS_01385168

%Fly3100P.DeviceDesc%	= LVCap138EA.Device, PCI\VEN_1131&DEV_7134&SUBSYS_01365168
%FlyDV3000P.DeviceDesc%	= LVCap138EA.Device, PCI\VEN_1131&DEV_7134&SUBSYS_01375168
%Fly3000P.DeviceDesc%	= LVCap138EA.Device, PCI\VEN_1131&DEV_7134&SUBSYS_01385168

%Fly3100N.DeviceDesc%	= LVCap138ES.Device, PCI\VEN_1131&DEV_7133&SUBSYS_01365168
%FlyDV3000N.DeviceDesc%	= LVCap138ES.Device, PCI\VEN_1131&DEV_7133&SUBSYS_01375168
%Fly3000N.DeviceDesc%	= LVCap138ES.Device, PCI\VEN_1131&DEV_7133&SUBSYS_01385168

%miniPCITVCard%		= LVCap138ES.Device, PCI\VEN_1131&DEV_7130&SUBSYS_02101043
%miniPCITVCard%		= LVCap138ES.Device, PCI\VEN_1131&DEV_7133&SUBSYS_02101043
%miniPCITVCard%		= LVCap138ES.Device, PCI\VEN_1131&DEV_7134&SUBSYS_02101043

%LVTuner.DeviceDesc%	= LVTuner.Device, STREAM\LVTUNER

;---------------------------------------------------------------
;			For LVCap138
;---------------------------------------------------------------
[LVCap138E.Device]
Include		= ks.inf, kscaptur.inf
Needs		= KS.Registration, KSCAPTUR.Registration
AddReg		= SAA713x.AddReg, LVCap138.AddReg, SAA7130.AddReg, Phi713x.34COM.AddReg
CopyFiles	= LVCap138.CopyDrivers, Phi713x.CopyFiles
KnownFiles	= LVCap138.KnownFiles

[LVCap138E.Device.NT]
Include		= ks.inf, kscaptur.inf
Needs		= KS.Registration, KSCAPTUR.Registration.NT
AddReg		= SAA713x.AddReg, LVCap138.AddReg, SAA7130.AddReg
RegisterDlls= Phi713x.34COM.Register
CopyFiles	= LVCap138.CopyDrivers, Phi713x.CopyFiles
KnownFiles	= LVCap138.KnownFiles

[LVCap138EA.Device]
Include		= ks.inf, kscaptur.inf
Needs		= KS.Registration, KSCAPTUR.Registration
AddReg		= SAA713x.AddReg, SAA7134.AddReg, SAA7133_4.AddReg, LVCap138.AddReg, Phi713x.Prop.AddReg, Phi713x.34COM.AddReg
CopyFiles	= LVCap138.CopyDrivers, Phi713x.CopyFiles
KnownFiles	= LVCap138.KnownFiles

[LVCap138EA.Device.NT]
Include		= ks.inf, kscaptur.inf
Needs		= KS.Registration, KSCAPTUR.Registration.NT
AddReg		= SAA713x.AddReg, SAA7134.AddReg, SAA7133_4.AddReg, LVCap138.AddReg
RegisterDlls= Phi713x.Prop.Register, Phi713x.34COM.Register
CopyFiles	= LVCap138.CopyDrivers, Phi713x.CopyFiles
KnownFiles	= LVCap138.KnownFiles

[LVCap138ES.Device]
Include		= ks.inf, kscaptur.inf
Needs		= KS.Registration, KSCAPTUR.Registration
AddReg		= SAA713x.AddReg, SAA7133.AddReg, SAA7133_4.AddReg, LVCap138.AddReg,Phi713x.Prop.AddReg, Phi713x.34COM.AddReg
CopyFiles	= LVCap138.CopyDrivers, Phi713x.CopyFiles
KnownFiles	= LVCap138.KnownFiles

[LVCap138ES.Device.NT]
Include		= ks.inf, kscaptur.inf
Needs		= KS.Registration, KSCAPTUR.Registration.NT
AddReg		= SAA713x.AddReg, SAA7133.AddReg, SAA7133_4.AddReg, LVCap138.AddReg
RegisterDlls= Phi713x.Prop.Register, Phi713x.34COM.Register
CopyFiles	= LVCap138.CopyDrivers, Phi713x.CopyFiles
KnownFiles	= LVCap138.KnownFiles

[LVCap138E.Device.NT.Services]
AddService	= LVCap138,0x00000002,LVCap138.ServiceInstall

[LVCap138E.Device.Interfaces]
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",LVCap138.Iface.Capture
AddInterface=%KSCATEGORY_VIDEO%,"GLOBAL",LVCap138.Iface.Capture
AddInterface=%KSCATEGORY_TVAUDIO%,"GLOBAL",LVCap138.Iface.TVAudio
AddInterface=%KSCATEGORY_CROSSBAR%,"GLOBAL",LVCap138.Iface.Crossbar

[LVCap138E.Device.NT.Interfaces]
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",LVCap138.Iface.Capture
AddInterface=%KSCATEGORY_VIDEO%,"GLOBAL",LVCap138.Iface.Capture
AddInterface=%KSCATEGORY_TVAUDIO%,"GLOBAL",LVCap138.Iface.TVAudio
AddInterface=%KSCATEGORY_CROSSBAR%,"GLOBAL",LVCap138.Iface.Crossbar

[LVCap138EA.Device.NT.Services]
AddService	= LVCap138,0x00000002,LVCap138.ServiceInstall

[LVCap138EA.Device.Interfaces]
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",LVCap138.Iface.Capture
AddInterface=%KSCATEGORY_VIDEO%,"GLOBAL",LVCap138.Iface.Capture
AddInterface=%KSCATEGORY_TVAUDIO%,"GLOBAL",LVCap138.Iface.TVAudio
AddInterface=%KSCATEGORY_CROSSBAR%,"GLOBAL",LVCap138.Iface.Crossbar

[LVCap138EA.Device.NT.Interfaces]
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",LVCap138.Iface.Capture
AddInterface=%KSCATEGORY_VIDEO%,"GLOBAL",LVCap138.Iface.Capture
AddInterface=%KSCATEGORY_TVAUDIO%,"GLOBAL",LVCap138.Iface.TVAudio
AddInterface=%KSCATEGORY_CROSSBAR%,"GLOBAL",LVCap138.Iface.Crossbar

[LVCap138ES.Device.NT.Services]
AddService	= LVCap138,0x00000002,LVCap138.ServiceInstall

[LVCap138ES.Device.Interfaces]
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",LVCap138.Iface.Capture
AddInterface=%KSCATEGORY_VIDEO%,"GLOBAL",LVCap138.Iface.Capture
AddInterface=%KSCATEGORY_TVAUDIO%,"GLOBAL",LVCap138.Iface.TVAudio
AddInterface=%KSCATEGORY_CROSSBAR%,"GLOBAL",LVCap138.Iface.Crossbar

[LVCap138ES.Device.NT.Interfaces]
AddInterface=%KSCATEGORY_CAPTURE%,"GLOBAL",LVCap138.Iface.Capture
AddInterface=%KSCATEGORY_VIDEO%,"GLOBAL",LVCap138.Iface.Capture
AddInterface=%KSCATEGORY_TVAUDIO%,"GLOBAL",LVCap138.Iface.TVAudio
AddInterface=%KSCATEGORY_CROSSBAR%,"GLOBAL",LVCap138.Iface.Crossbar

[LVCap138.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,lvcap138.sys
HKR,,PageOutWhenUnopened,3,0
HKR,,DontSuspendIfStreamsAreRunning,3,00

; Registry Settings for LR138 Adapter
HKR, "Decoder", "Tuner Channel",0x00010001,1
HKR, "Decoder", "CVBS Channel",0x00010001,3
HKR, "Decoder", "SVHS Channel",0x00010001,6

HKR, "BoardSetting", "Composite1",0x00010001,3
HKR, "BoardSetting", "SVideo1",0x00010001,3
HKR, "BoardSetting", "FM", 0x00010001, 3

HKR, "Audio", "VoltageInputSelect", 0x00010001, 1

HKR, "Parameters", "VideoTunerEnabled",0x00010001,1
HKR, "Parameters", "SVideoEnabled",0x00010001,1
HKR, "Parameters", "CompositeEnabled",0x00010001,1
HKR, "Parameters", "FMSupported", 0x00010001, 0x01
HKR, "Parameters", "CapPreviewEnabled", 0x00010001, 0x01

; Insert the appropriate preferred video standard here.
; If no video standard can be detected (e.g. if no
; video source is connected), this standard is assumed:
;   KS_AnalogVideo_PAL_B    = 0x00000010
;   KS_AnalogVideo_NTSC_M   = 0x00000001
;   KS_AnalogVideo_NTSC_M_J = 0x00000002
;   see Windows DDK for other video standards
HKR, "Decoder", "Preferred Video Standard",0x00010001,0x00000010    ; KS_AnalogVideo_PAL_B
; Insert the default VBI sampling frequency and line length here.
HKR, "Decoder", "VBI Sampling Frequency",0x00010001,27000000
HKR, "Decoder", "VBI Pitch",0x00010001,1440

; 07.08.2003 removed the LVREMOTE
HKR, "ENUM\Device1",pnpid,,LVTUNER

; Common registry entries for SAA7134 and SAA7130
; Update this field from Philips Infs
[SAA713x.AddReg]
;>>> decoder defaults for tuner input
HKR, "Decoder\SRC1", "Video Standard",0x00010001,0x20
HKR, "Decoder\SRC1", "Brightness",0x00010001,0x80
HKR, "Decoder\SRC1", "Contrast",0x00010001,0x44
HKR, "Decoder\SRC1", "Saturation",0x00010001,0x40
HKR, "Decoder\SRC1", "HUE",0x00010001,0x00
HKR, "Decoder\SRC1", "Sharpness",0x00010001,0x00
HKR, "Decoder\SRC1", "Source Type",0x00010001,0x01
HKR, "Decoder\SRC1", "Y-Filter",0x00010001,0x01
HKR, "Decoder\SRC1", "C-Filter",0x00010001,0x01
HKR, "Decoder\SRC1", "C-Bypass",0x00010001,0x00

;>>>  decoder defaults for composite 1 source
HKR, "Decoder\SRC0", "Video Standard",0x00010001,0x20
HKR, "Decoder\SRC0", "Brightness",0x00010001,0x80
HKR, "Decoder\SRC0", "Contrast",0x00010001,0x44
HKR, "Decoder\SRC0", "Saturation",0x00010001,0x40
HKR, "Decoder\SRC0", "HUE",0x00010001,0x00
HKR, "Decoder\SRC0", "Sharpness",0x00010001,0x00
HKR, "Decoder\SRC0", "Source Type",0x00010001,0x02
HKR, "Decoder\SRC0", "Y-Filter",0x00010001,0x01
HKR, "Decoder\SRC0", "C-Filter",0x00010001,0x01
HKR, "Decoder\SRC0", "C-Bypass",0x00010001,0x00

;>>>  decoder defaults for composite 2 source
HKR, "Decoder\SRC2", "Video Standard",0x00010001,0x20
HKR, "Decoder\SRC2", "Brightness",0x00010001,0x80
HKR, "Decoder\SRC2", "Contrast",0x00010001,0x44
HKR, "Decoder\SRC2", "Saturation",0x00010001,0x40
HKR, "Decoder\SRC2", "HUE",0x00010001,0x00
HKR, "Decoder\SRC2", "Sharpness",0x00010001,0x00
HKR, "Decoder\SRC2", "Source Type",0x00010001,0x02
HKR, "Decoder\SRC2", "Y-Filter",0x00010001,0x01
HKR, "Decoder\SRC2", "C-Filter",0x00010001,0x01
HKR, "Decoder\SRC2", "C-Bypass",0x00010001,0x00

;>>>  decoder defaults for SVHS source
HKR, "Decoder\SRC3", "Video Standard",0x00010001,0x20
HKR, "Decoder\SRC3", "Brightness",0x00010001,0x80
HKR, "Decoder\SRC3", "Contrast",0x00010001,0x44
HKR, "Decoder\SRC3", "Saturation",0x00010001,0x40
HKR, "Decoder\SRC3", "HUE",0x00010001,0x00
HKR, "Decoder\SRC3", "Sharpness",0x00010001,0x00
HKR, "Decoder\SRC3", "Source Type",0x00010001,0x02
HKR, "Decoder\SRC3", "Y-Filter",0x00010001,0x00
HKR, "Decoder\SRC3", "C-Filter",0x00010001,0x00
HKR, "Decoder\SRC3", "C-Bypass",0x00010001,0x01

; 'I2S Output' reflects the state of the two I2S output channels (1=enabled/0=disabled)
HKR, "Audio", "I2S Output",0x00010001,0x00
HKR, "Audio", "I2S2 Output",0x00010001,0x00


;Registry entries for SAA7130
[SAA7130.AddReg]
;HKR, "Parameters", "CapAudioEnabled",0x00010001,0          ; diable audio capture pin
HKR, "BoardSetting", "Tuner",0x00010001,3

;Registry entries for SAA7134
[SAA7134.AddReg]
HKR, "BoardSetting", "Tuner",0x00010001,1			; use Audio DSP
;>>> audio settings for tuner input
; 'CountryCode' reflects the used Country
; and is used as a table entry to 'DefaultStandard' and 'StandardTable'
; in order to perform a country dependant audio standard search
; _OEM_  Enter the appropriate country code here
HKR, "", "CountryCode",,"49"   ; Germany
; 'XTAL' reflects the used hardware crystal (0=32.11MHz,1=24.567MHz)
HKR, "Audio", "XTAL",0x00010001,0x01
; 'DetectMode' reflects the used audio detection mode (1=automatic mode,0=manual mode)
HKR, "Audio", "DetectMode",0x00010001,0x01          ; automatic mode

;Registry entries for SAA7133
[SAA7133.AddReg]
HKR, "BoardSetting", "Tuner",0x00010001,1			; use Audio DSP
; 'CountryCode' reflects the used Country
; and is used as a table entry to 'DefaultStandard' and 'StandardTable'
; in order to perform a country dependant audio standard search
HKR, "", "CountryCode",,"49"     ; Germany

; 'XTAL' reflects the used hardware crystal (0=32.11MHz,1=24.567MHz)
HKR, "Audio", "XTAL",0x00010001,0x01
; 'DetectMode' reflects the used audio detection mode (1=automatic mode,0=manual mode)
HKR, "Audio", "DetectMode",0x00010001,0x01
; 'Voltage Input Select' defines the input voltage of the 2 external inputs (0=1.0 Vrms/1=2.0 Vrms)
HKR, "Audio", "Voltage Input Select Ext1",0x00010001,0x00
HKR, "Audio", "Voltage Input Select Ext2",0x00010001,0x00
; 'Virtual Stereo Effect' is the pre-defined width of 'Philips Incredible Stereo' (0=narrow...5=wide)
HKR, "Audio", "Virtual Stereo Effect",0x00010001,0x04
; Audio master clock settings
HKR, "Audio", "MClk Output Enable",0x00010001,0x0
HKR, "Audio", "MClk Frequency",0x00010001,0x0
HKR, "Audio", "MClk Reference Switch",0x00010001,0x0
HKR, "Audio", "MClk Reference Divider",0x00010001,0x2

; Registry entries for SAA7133/4
[SAA7133_4.AddReg]
; possible 'software' audio enable/disable switch (0=disable,1=enable) 
HKR, "Parameters", "AudioEnabled",0x00010001,1          ; enable audio
HKR, "Parameters", "AudioTunerEnabled",0x00010001,1     ; enable tuner audio

; 'DefaultStandard'
; in automatic mode: 'DefaultStandard' is used as a fallback if nothing is detected
; in manual mode:    'DefaultStandard' is used as standard to be set
;   2  = B/G   Mono           
;   3  = D/K   Mono           
;   4  = M     Mono           
;   5  = B/G   A2
;   6  = B/G   Nicam
;   7  = D/K   A2 Type 1
;   8  = D/K   A2 Type 2
;   9  = D/K   A2 Type 3
;   10 = D/K   Nicam
;   11 = L/L'  Nicam
;   12 = L/L'  AM
;   13 = I     Nicam
;   14 = I     Mono
;   15 = M     Korea
;   16 = M     BTSC
HKR, "Audio\DefaultStandard", "01",0x00010001,16   ; USA:           M    BTSC
HKR, "Audio\DefaultStandard", "31",0x00010001,5    ; Netherlands:   B/G  A2
HKR, "Audio\DefaultStandard", "32",0x00010001,6    ; Belgium:       B/G  Nicam
HKR, "Audio\DefaultStandard", "33",0x00010001,11   ; France:        L/L' Nicam
HKR, "Audio\DefaultStandard", "34",0x00010001,5    ; Spain:         B/G  A2
HKR, "Audio\DefaultStandard", "39",0x00010001,5    ; Italy:         B/G  A2
HKR, "Audio\DefaultStandard", "41",0x00010001,5    ; Switzerland:   B/G  A2
HKR, "Audio\DefaultStandard", "44",0x00010001,13   ; Great Britain: I    Nicam
HKR, "Audio\DefaultStandard", "45",0x00010001,6    ; Denmark        B/G  Nicam
HKR, "Audio\DefaultStandard", "46",0x00010001,6    ; Sweden:        B/G  Nicam
HKR, "Audio\DefaultStandard", "47",0x00010001,6    ; Norway:        B/G  Nicam
HKR, "Audio\DefaultStandard", "49",0x00010001,5    ; Germany:       B/G  A2
HKR, "Audio\DefaultStandard", "81",0x00010001,16   ; Japan:         M    BTSC
HKR, "Audio\DefaultStandard", "86",0x00010001,7    ; China:         D/K  A2 Type 1
HKR, "Audio\DefaultStandard","351",0x00010001,5    ; Azores:        B/G  A2
HKR, "Audio\DefaultStandard","358",0x00010001,6    ; Finland:       B/G  Nicam
HKR, "Audio\DefaultStandard","420",0x00010001,10   ; Czech Republic:D/K  Nicam

; 'StandardTable'
; in automatic mode: StandardTable is used to set the standard groups to be searched
; bit array:
;   bit1 = B/G
;   bit2 = D/K
;   bit3 = L/L'
;   bit4 = I
;   bit5 = M
HKR, "Audio\StandardTable", "01",0x00010001,0x10   ; USA:           M
HKR, "Audio\StandardTable", "31",0x00010001,0x01   ; Netherlands:   B/G
HKR, "Audio\StandardTable", "32",0x00010001,0x01   ; Belgium:       B/G
HKR, "Audio\StandardTable", "33",0x00010001,0x04   ; France:        L/L'
HKR, "Audio\StandardTable", "34",0x00010001,0x01   ; Spain:         B/G
HKR, "Audio\StandardTable", "39",0x00010001,0x01   ; Italy:         B/G
HKR, "Audio\StandardTable", "41",0x00010001,0x01   ; Switzerland:   B/G
HKR, "Audio\StandardTable", "44",0x00010001,0x08   ; Great Britain: I
HKR, "Audio\StandardTable", "45",0x00010001,0x01   ; Denmark        B/G
HKR, "Audio\StandardTable", "46",0x00010001,0x01   ; Sweden:        B/G
HKR, "Audio\StandardTable", "47",0x00010001,0x01   ; Norway:        B/G
HKR, "Audio\StandardTable", "49",0x00010001,0x01   ; Germany:       B/G
HKR, "Audio\StandardTable", "81",0x00010001,0x10   ; Japan:         M
HKR, "Audio\StandardTable", "86",0x00010001,0x02   ; China:         D/K
HKR, "Audio\StandardTable","351",0x00010001,0x01   ; Azores:        B/G
HKR, "Audio\StandardTable","358",0x00010001,0x01   ; Finland:       B/G
HKR, "Audio\StandardTable","420",0x00010001,0x02   ; Czech Republic:D/K

[LVCap138.CopyDrivers]
lvcap138.sys

[LVCap138.KnownFiles]
lvcap138.sys	= safe

[LVCap138.ServiceInstall]
DisplayName   = %LVCap138.ServiceName%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %12%\lvcap138.sys

[LVCap138.Iface.Capture]
AddReg=LVCap138.Iface.Capture.AddReg 

[LVCap138.IFace.TVAudio]
AddReg=LVCap138.Iface.TVAudio.AddReg

[LVCap138.Iface.Crossbar]
AddReg=LVCap138.Iface.Crossbar.AddReg

[LVCap138.Iface.Capture.AddReg]
HKR,,CLSID,,%CLSID_Proxy%
HKR,,FriendlyName,,%LVCap138.Iface.Capture.Desc%

;Philips Dlls
HKLM,SOFTWARE\Intel\Intercast\TVControl,TVControlDLL,,34TVCtrl.dll
HKLM,SOFTWARE\Intel\Intercast\Drivers,biBitCount,,16
HKLM,SOFTWARE\Intel\Intercast\Drivers,biCompression,,BI_RGB
HKLM,SOFTWARE\Intel\Intercast\Drivers,Capture Description,,%LVCap138.Iface.Capture.Desc%
HKCR,Intercast.Display,DisplayBitMask,,f


; Private Pin Names:
; MEDIATYPE_Audio:
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\{73647561-0000-0010-8000-00AA00389B71},"Name",0x00000000,"Audio"
; GUID_VSB_OUT:
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\{F3954424-34F6-11D1-821D-0000F8300212},"Name",0x00000000,"Transport In"
; MEDIUM_AUDIO_PHILDEC_ANALOGAUDIOIN:
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\{0482DEE1-7817-11cf-8a03-00aa006ecb65},"Name",0x00000000,"Analog Audio In"

[LVCap138.Iface.TVAudio.AddReg]
HKR,,CLSID,,%CLSID_TVAudioFilter%
HKR,,FriendlyName,,%LVCap138.Iface.TVAudio.Desc%

[LVCap138.Iface.CrossBar.AddReg]
HKR,,CLSID,,%CLSID_CrossBarFilter%
HKR,,FriendlyName,,%LVCap138.Iface.Crossbar.Desc%

[Phi713x.CopyFiles]
34api.dll
34pciurd.dll
34i2curd.dll
34dd.dll
34ds.dll
34dialog.dll
34dlg2.dll
34TvCtrl.dll
34com.dll
Prop7134.dll      ; audio property dialog

[Phi713x.Prop.AddReg]
HKLM,Software\Microsoft\Windows\CurrentVersion\RunOnce,"AudioProperties",,"%11%\Regsvr32 /s %11%\Prop7134.dll"

[Phi713x.34COM.AddReg]
HKLM,Software\Microsoft\Windows\CurrentVersion\RunOnce,"COMInterface",,"%11%\Regsvr32 /s %11%\34com.dll"

[Phi713x.Prop.Register]
11,,Prop7134.dll,1 ;FLG_REGSVR_DLLREGISTER

[Phi713x.34COM.Register]
11,,34COM.dll,1 ;FLG_REGSVR_DLLREGISTER

;---------------------------------------------------------------
;			For LVTuner
;---------------------------------------------------------------
[LVTuner.Device]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration
AddReg     = LVTuner.AddReg
CopyFiles  = LVTuner.CopyDrivers
KnownFiles = LVTuner.KnownFiles

[LVTuner.Device.NT]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration.NT
AddReg     = LVTuner.AddReg
CopyFiles  = LVTuner.CopyDrivers
KnownFiles = LVTuner.KnownFiles

[LVTuner.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,lvtuner.sys
HKR,,PageOutWhenUnopened,3,0

[LVTuner.CopyDrivers]
lvtuner.sys 

[LVTuner.KnownFiles]
lvtuner.sys	= Safe

[LVTuner.Device.NT.Services]
AddService	= lvtuner,0x00000002,LVTuner.ServiceInstall

[LVTuner.ServiceInstall]
DisplayName   = %LVTuner.DeviceDesc%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %12%\lvtuner.sys

[LVTuner.Device.Interfaces]
AddInterface	= %KSCATEGORY_TVTUNER%,"GLOBAL",LVTuner.Iface.Tuner,

[LVTuner.Device.NT.Interfaces]
AddInterface	= %KSCATEGORY_TVTUNER%,"GLOBAL",LVTuner.Iface.Tuner,

[LVTuner.Iface.Tuner]
AddReg	= LVTuner.Iface.Tuner.AddReg

[LVTuner.Iface.Tuner.AddReg]
HKR,,CLSID,,%CLSID_CTVTunerFilter%
HKR,,FriendlyName,,%LVTuner.Iface.Tuner.Desc%


;---------------------------------------------------------------
;                S t r i n g s
;---------------------------------------------------------------
[Strings]

;----------------
; Non-Localizable
;----------------

SERVICE_KERNEL_DRIVER	= 1
SERVICE_ERROR_NORMAL	= 1
SERVICE_AUTO_START	= 2
SERVICE_DEMAND_START	= 3

KSCATEGORY_CROSSBAR	= {a799a801-a46d-11d0-a18c-00a02401dcd4}
KSCATEGORY_CAPTURE	= {65e8773d-8f56-11d0-a3b9-00a0c9223196}
KSCATEGORY_VIDEO	= {6994AD05-93EF-11D0-A3CC-00A0C9223196}
KSCATEGORY_TVTUNER	= {a799a800-a46d-11d0-a18c-00a02401dcd4}
KSCATEGORY_TVAUDIO	= {a799a802-a46d-11d0-a18c-00a02401dcd4}

CLSID_Proxy		= {17CCA71B-ECD7-11D0-B908-00A0C9223196}
CLSID_TVAudioFilter	= {71F96462-78F3-11d0-A18C-00A0C9118956}
CLSID_CrossBarFilter	= {71F96460-78F3-11d0-A18C-00A0C9118956}
CLSID_CTVTunerFilter	= {266EEE40-6C63-11cf-8A03-00AA006ECB65}

;----------------
;	   OEM
;----------------
CAPDRV.SYS  = lvcap138.sys
TVTUNER.SYS = lvtuner.sys

;07.08.2003 removed the LVREMOTE
TVTUNER.DRV.ID	= LVTUNER

;----------------
; Localizable
;----------------
Lifeview	= "TV Card WDM Video Capture"
Disk1		= "TV Card WDM Video Capture"

LVCap138.ServiceName	= "TV Card WDM Video Capture"

Fly2100.DeviceDesc	= "TV Card 7130 LP"
FlyDV2000.DeviceDesc	= "DV Card 7130"
Fly2000.DeviceDesc	= "TV Card 7130"

Fly3100P.DeviceDesc	= "TV Card 7134 LP"
FlyDV3000P.DeviceDesc	= "DV Card 7134"
Fly3000P.DeviceDesc	= "TV Card 7134"

Fly3100N.DeviceDesc	= "TV Card 7133 LP"
FlyDV3000N.DeviceDesc	= "DV Card 7133"
Fly3000N.DeviceDesc	= "TV Card 7133"

FlyVideo2100.DeviceDesc		= "TV Card 7130"
FlyVideo2000.DeviceDesc		= "TV Card 7130"

FlyVideo3100N.DeviceDesc	= "TV Card 7134"
FlyVideo3000N.DeviceDesc	= "TV Card 7134"

FlyVideo3100P.DeviceDesc	= "TV Card 7134"
FlyVideo3000P.DeviceDesc	= "TV Card 7134"

miniPCITVCard		= "MiniPCI TV CARD"

LVCap138.Iface.Capture.Desc	= "TV Card WDM Video Capture"
LVCap138.Iface.TVAudio.Desc	= "TV Card TV Audio"
LVCap138.Iface.CrossBar.Desc	= "TV Card CrossBar"

LVTuner.DeviceDesc		= "TV Card TV Tuner"
LVTuner.Iface.Tuner.Desc	= "TV Card TV Tuner"
