USER'S MANUAL(English Version)
1: Introduce
   USB2.0 to SATA/IDE Cable be used to connect Hard disk,
   CD-ROM,DVD-ROM,CD-RW,COMBO device,
   DVD-RW to computer with USB 2.0 interface.
2: Features
   USB 2.0 supports 480M data transfer rate and 52X
   CDROM data read. External power supply can be use
   to AC90-264V,47-63Hz.
3: Components
   1. USB to SATA/IDE cable: used to connect SATA/IDE
   device to computer with USB port.
   2.Power with 12V and 5V double channel output:
   used to supply power to SATA/IDE device.
4: Package
   USB to SATA/IDE cable    1Pcs
   AC Power                 1Pcs
   Driver CD                1pcs
5: Device Installation
   Hardware install:
   1. Comfirm device is under master mode.
   2. Connect SATA/IDE connect to SATA/IDE device.
   3. Connect AC power to SATA/IDE device.
   4. Connect cable to USB port of computer.
Drive Install
   1. Windows98: Insert Driver CD to CDROM and run X:\win98\setup.exe 
      before you insert the cable to your computer.
   2. Windows 2000/me/XP: you don't need to install any driver
   3. Mac8.6 or higher:
      Copy gene USB SATA/IDE_05E3_0702.sit to desktop and double click 
      it to get driver file. Then copy the driver file to [System Folder]
      [Extensions]. after that,connect cable to computer and reboot the system.
6: Uninstall
   1. Click the hot swap icon on the task column with right button of the mouse,
      and stop the device.
   2. Pull out the cable.
   3. Pull out the power supply.





