[Version]
Signature="$CHICAGO$"
Class=HDC
provider=%MSFT%

[Manufacturer]
%MfgName%=Microsoft

[Microsoft]
%DeviceDesc%=JMUSB.install,USB\VID_152D&PID_2338
%JMUS\DISK.DeviceDesc%=jmuspdr.install,USBSTOR\JMDISK

[PreCopySection]
HKR,,NoSetupUI,,1

[DestinationDirs]
jmus.files = 10,System32\Drivers
jmuspdr.files = 12

[JMUSB.install]
CopyFiles=jmus.files, jmuspdr.files
AddReg=jmus.addreg

[Sandisk.install]
CopyFiles=jmus.files, jmuspdr.files
AddReg=jmus.addreg

[ImationLS120.install]
CopyFiles=jmus.files, jmuspdr.files
AddReg=jmus.addreg

[ImationLS120.install.HW]
AddReg=cb.addreg.HW

[jmus.addreg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,jmusbsto.SYS


; If the device does not correctly indicate which protocol it uses,
; one of the following sections should be added to indicate which protocol
; the driver should use.

; Indicate that the device uses the C/B/I protocol
[cbi.addreg.HW]
HKR,,DeviceProtocol,0x10001,00

; Indicate that the device uses the C/B protocol
[cb.addreg.HW]
HKR,,DeviceProtocol,0x10001,01

; Indicate that the device uses the BULK ONLY protocol
[bulkonly.addreg.HW]
HKR,,DeviceProtocol,0x10001,50

; Install the port driver
[jmuspdr.install]
AddReg=jmuspdr.addreg

[jmuspdr.addreg]
HKR,,DevLoader,,*ios
HKR,,PortDriver,,jmuspdr.pdr
HKLM,%AUTORUN%,JMUsbMon,,"JMUsbMon.exe"


[jmus.files]
jmusbsto.sys

[jmuspdr.files]
jmuspdr.pdr

[SourceDisksNames]
1000 = "USB Mass Storage Driver Disk","",,

[SourceDisksFiles]
jmusbsto.SYS = 1000
jmusPDR.PDR = 1000

;---------------------------------------------------------------;

[Strings]
MSFT="JMicron"
MfgName="JMicron"
DeviceDesc="JM20338 SATA, USB Combo"
jmus\DISK.DeviceDesc="USB Mass Storage Device"
AUTORUN="Software\Microsoft\Windows\CurrentVersion\Run"
