**
**                                   
** VIA Rhine Family Fast Ethernet Adapter
** 
** FETNWSRV.INF
** 
** v4.02    Dec. 2001
**
**

[version]
InfVersion=00.01.00
signature=$CHICAGO$
Class=Net
provider=%V_N%

;****************************************************************************
;       Manufacturer Section
;****************************************************************************
[Manufacturer]
%V_MAN%=VIA

;****************************************************************************
;       Manufacturer Name Section
;****************************************************************************
[VIA]
%*fetnwsrv.DeviceDesc%=*fetnwsrv.Ndi,        PCI\VEN_1106&DEV_3106 ; fetnwsrv

;****************************************************************************
;       INF INSTALL SECTION
;****************************************************************************
[*fetnwsrv.Ndi]
AddReg=*fetnwsrv.Ndi.reg, via3043.Ndi.reg, ODI.Common.CFG.reg

;****************************************************************************
;       Registerry (device id and vendor id)
;****************************************************************************
[*fetnwsrv.Ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_1106&DEV_3106"

;****************************************************************************
;       Register Common Settings for all VIA drivers
;****************************************************************************
[via3043.Ndi.reg]
; key,subkey,valuname,type,value
HKR,,DevLoader,,*odiload
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"

; Ndi section
HKR,Ndi,NdiInstaller,,"odipage.dll,odiNdiproc"

; Interfaces
HKR,Ndi\Interfaces,DefUpper,,"odinsup,NovellODI32"
HKR,Ndi\Interfaces,UpperRange,,"odinsup,NovellODI32"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"

; Install section
HKR,Ndi\Install,"16 Bit",,"via3043.ODI16.Install"
HKR,Ndi\Install,"32 Bit",,"via3043.ODI32.Install"

; Remove section
HKR,Ndi\Remove,"16 Bit",,"via3043.ODI16.Remove"

; ODI 16 Bit info
HKR,"ODI\16 Bit",ModulePath,,"%24%%DRIVER_32_PATH%"
HKR,"ODI\16 Bit",Modules,,"LSLC32.NLM,PC32MLID.LAN"
HKR,"ODI\16 Bit",DriverPath,,"%24%%DRIVER_16_PATH%"
HKR,"ODI\16 Bit",NetcfgPath,,"%24%%DRIVER_16_PATH%"
HKR,"ODI\16 Bit",NetcfgFileName,,"Net.cfg"
HKR,"ODI\16 Bit",FileName,,"fetodi.com"
HKR,"ODI\16 Bit",LinkDriver,,"fetodi"

; ODI 32 Bit Info
HKR,"ODI\32 Bit",ModulePath,,"%24%%DRIVER_32_PATH%"
HKR,"ODI\32 Bit",Modules,,"LSLC32.NLM,CMSM.NLM,ETHERTSM.NLM"
HKR,"ODI\32 Bit",DriverPath,,"%24%%DRIVER_32_PATH%"
HKR,"ODI\32 Bit",FileName,,"fetnwsrv.lan"

;****************************************************************************
;       Install Section
;****************************************************************************
[via3043.ODI16.Install]
CopyFiles=via3043.ODI16.CopyFiles
UpdateAutoBat=via3043.ODI16.autobat

[via3043.ODI32.Install]
CopyFiles=via3043.ODI32.CopyFiles
UpdateAutoBat=via3043.ODI32.autobat

[via3043.ODI16.autobat]
CmdDelete=LSL
CmdDelete=N16ODI
CmdDelete=NESL
CmdDelete=fetodi             ; 11.11.96
CmdDelete=ODIHLP
CmdAdd=LSL.COM,  "-c=%24%%DRIVER_16_PATH%NET.CFG"
CmdAdd=N16ODI.COM
CmdAdd=NESL.COM
CmdAdd=fetodi.COM

[via3043.ODI32.autobat]
CmdDelete=LSL
CmdDelete=N16ODI
CmdDelete=NESL
CmdDelete=fetnwsrv
CmdDelete=ODIHLP

;****************************************************************************
;       Remove Section
;****************************************************************************
[via3043.ODI16.Remove]
UpdateAutoBat=via3043.ODI16.AutoBatRemove

[via3043.ODI16.AutoBatRemove]
CmdDelete=LSL
CmdDelete=N16ODI
CmdDelete=NESL
CmdDelete=fetodi

;****************************************************************************
;       general Ethernet Frame-Type params
;****************************************************************************
[ODI.Common.CFG.reg]
; First Logical Board
HKR,Ndi\params\Frame1,ParamDesc,,"1. Frame Type"
HKR,Ndi\params\Frame1,default,,1
HKR,Ndi\params\Frame1,type,,enum
HKR,Ndi\params\Frame1,optional,,0
HKR,Ndi\params\Frame1\enum,1,,"Ethernet_802.2"
HKR,Ndi\params\Frame1\enum,2,,"Ethernet_SNAP"
HKR,Ndi\params\Frame1\enum,3,,"Ethernet_II"
HKR,Ndi\params\Frame1\enum,4,,"Ethernet_802.3"

; Second Logical Board
HKR,Ndi\params\Frame2,ParamDesc,,"2. Frame Type"
HKR,Ndi\params\Frame2,default,,2
HKR,Ndi\params\Frame2,type,,enum
HKR,Ndi\params\Frame2,optional,,0
HKR,Ndi\params\Frame2\enum,1,,"Ethernet_802.2"
HKR,Ndi\params\Frame2\enum,2,,"Ethernet_SNAP"
HKR,Ndi\params\Frame2\enum,3,,"Ethernet_II"
HKR,Ndi\params\Frame2\enum,4,,"Ethernet_802.3"
HKR,Ndi\params\Frame2\enum,5,,"Not used"

; Third Logical Board
HKR,Ndi\params\Frame3,ParamDesc,,"3. Frame Type"
HKR,Ndi\params\Frame3,default,,3
HKR,Ndi\params\Frame3,type,,enum
HKR,Ndi\params\Frame3,optional,,0
HKR,Ndi\params\Frame3\enum,1,,"Ethernet_802.2"
HKR,Ndi\params\Frame3\enum,2,,"Ethernet_SNAP"
HKR,Ndi\params\Frame3\enum,3,,"Ethernet_II"
HKR,Ndi\params\Frame3\enum,4,,"Ethernet_802.3"
HKR,Ndi\params\Frame3\enum,5,,"Not used"

; Fourth Logical Board
HKR,Ndi\params\Frame4,ParamDesc,,"4. Frame Type"
HKR,Ndi\params\Frame4,default,,4
HKR,Ndi\params\Frame4,type,,enum
HKR,Ndi\params\Frame4,optional,,0
HKR,Ndi\params\Frame4\enum,1,,"Ethernet_802.2"
HKR,Ndi\params\Frame4\enum,2,,"Ethernet_SNAP"
HKR,Ndi\params\Frame4\enum,3,,"Ethernet_II"
HKR,Ndi\params\Frame4\enum,4,,"Ethernet_802.3"
HKR,Ndi\params\Frame4\enum,5,,"Not used"

; Node Address Override
HKR,Ndi\params\"Node Address",ParamDesc,,"Node Address Override"
HKR,Ndi\params\"Node Address",type,,edit
HKR,Ndi\params\"Node Address",LimitText,,18
HKR,Ndi\params\"Node Address",UpperCase,,1
HKR,Ndi\params\"Node Address",default,,""
HKR,Ndi\params\"Node Address",flag,1,20,00,00,00
HKR,Ndi\params\"Node Address",optional,,1

; W95flag
;HKR,Ndi\params\W95flag,ParamDesc,,"W95flag"
;HKR,Ndi\params\W95flag,type,,keyonly
;HKR,Ndi\params\W95flag,optional,,0

; Help section
HKR,Ndi,HelpText,,%ODIMLID_HELP%

;****************************************************************************
; File to be copied
;****************************************************************************
[via3043.ODI32.CopyFiles]
FETNWSRV.LAN,,,5

[via3043.ODI16.CopyFiles]
fetodi.com,,,5
LSL.com,,,5
N16ODI.COM,,,5
NESL.COM,,,5
;LSL.msg,,,5
;NESL.msg,,,5

;****************************************************************************
; Source Disk Names & Source Disk Files
;****************************************************************************
[SourceDisksNames]
42=%DSK_NOVELL%,"",0004

[SourceDisksFiles]
fetnwsrv.lan  =42
fetodi.com    =42
LSL.com       =42
N16ODI.COM    =42
NESL.COM      =42

;****************************************************************************
; Destination Directories
;****************************************************************************
[DestinatioNdirs]
DefaultDestDir               =11
via3043.ODI32.CopyFiles       =24,novell\client32
via3043.ODI16.CopyFiles       =24,novell\nwclient

;****************************************************************************
; Localizable Strings
;****************************************************************************
[strings]
; Provider
V_N=" Novell"

; Manufacturers
V_MAN="VIA"

;Paths to drivers
DRIVER_32_PATH="novell\client32\"
DRIVER_16_PATH="novell\nwclient\"
DSK_NOVELL="Novell NetWare Client-32 LAN driver disk"

; VIA Devices
*fetnwsrv.DeviceDesc="VIA Rhine Family Fast Ethernet Adapter for Netware Client-32"

; Context help
ODIMLID_HELP="The ODI 32-bit driver enables you to use either 16-Bit or 32-Bit networking components."
